PC ORG @ 0x1e + ! ( chkPS )
( Note that you only need to call this in words that push
  back to PSP. If they don't, calling chkPS is redundant with
  check in next )
    EXX,
( We have the return address for this very call on the stack
  and protected registers. 2 - is to compensate that. )
    HL PS_ADDR 2 - LDddnn,
    SP SUBHLss,
    EXX,
    CNC RETcc,      ( PS_ADDR >= SP? good )
    JR, L2 BWR      ( abortUnderflow-B298 )

