( handle backspace: go back one char in IN>, if possible, then
  emit BS + SPC + BS )
: (inbs)
    ( already at IN( ? )
    IN> @ IN( = IF EXIT THEN
    IN> @ 1- IN> !
    BS SPC BS
;

: KEY
    85 RAM+ @ ( (key) override )
    ?DUP IF EXECUTE ELSE (key) THEN ;


( cont.: read one char into input buffer and returns whether we
  should continue, that is, whether CR was not met. )
