: RAM+ [ RAMSTART LITN ] + ; : BIN+ [ BIN( @ LITN ] + ;
: HERE 0x04 RAM+ ;
: CURRENT* 0x51 RAM+ ; : CURRENT CURRENT* @ ;
: H@ HERE @ ;
: FIND ( w -- a f ) CURRENT @ SWAP _find ;
: IN> 0x30 RAM+ ; ( current position in INBUF )
: IN( 0x32 RAM+ @ ; ( points to INBUF )
: IN) 0x40 ( buffer size ) IN( + ; ( INBUF's end )
: (infl) 0 IN( DUP IN> ! ! ; ( flush input buffer )
: QUIT
    (resRS) 0 0x08 RAM+ ! ( C<* override ) (infl)
    LIT< (main) FIND DROP EXECUTE
;
1 25 LOADR+ ( xcomp core low )
