KEY overrides can be used to, for example, temporarily give
prompt control to a RS-232 device instead of the keyboard.

Interpreter output is unbuffered and only has EMIT. This
word can also be overriden, mostly as a companion to the
raison d'etre of your KEY override.
