(cont.)
OUT [nA, (C)r]         IN [An, r(C)]
SET [br]   RES [br]    BIT [br]
RL [r]     RLC [r]     SLA [r]     RLA         RLCA
RR [r]     RRC [r]     SRL [r]     RRA         RRCA
CALL [nn]  RST [n]     DJNZ
JP [nn, (HL), (IX), (IY)]
JR [, Z, NZ, C, NC]

DI         EI          EXDEHL      EXX         HALT
NOP        RET         RETI        RETN        SCF
